Electro-disintegration

— complicated input (responses as funcs of ω, θ_e, θ^{cm}_{pq} ) — different for each beam energy

— non-trivial smoothing — slow look-up

Electro-disintegration at θcmpq = 7.5∘

Spline problem